Default Interface File for Ad-Hoc

* sudo nano /etc/network/interfaces-adhoc

auto lo

iface lo inet loopback  
iface eth0 inet dhcp  
iface usb0 inet static

address 192.168.x.y  
netmask 255.255.255.0

allow-hotplug wlan0  
iface wlan0 inet static

wireless-channel 1  
wireless-essid RPiAdHocNetwork  
wireless-mode ad-hoc

* x and y must be set accordingly