Default Interface File for WiFi

* sudo nano /etc/network/interfaces

auto lo

iface lo inet loopback  
iface eth0 inet dhcp  
iface usb0 inet static

address 192.168.x.y  
netmask 255.255.255.0  
network 192.168.x.0  
broadcast 192.168.x.255

allow-hotplug wlan0  
iface wlan0 inet manual  
wpa-roam /etc/wpa\_supplicant/wpa\_supplicant.conf  
iface default inet dhcp

* x and y must be set accordingly