|  |  |
| --- | --- |
| **Issue:** | **Solution:** |
| Chariot moving around erratically left & right | Changed the – (minus) around in RcChan, for the motor output |
|  |  |
|  |  |
|  |  |

**Issues and Solutions**